Enigma-E  3D-Printed Keyboard

----------------------------------------------------
Print Keyboard cover
Printer Prusa MK4, Filament PLA Black
----------------------------------------------------

1. Print "Tastatur v3.3mf" 
Extruder 0.15mm, Infill: 15%,  Support: on support enforcer only
At about 25% of the printing, the print pauses and you must insert 2 Neodyn magnets 20x5x2mm then resume printing.
Remove the supports from the keyboard and clean up.
* Test: The keyboad shall already fit the Enigma-E.

2. Print "Button V5.3mf"
These are the key base for the upper row of the keyboard. There are 12  pieces but you need only 9 of them. The rest is for the case some thread does not fit or something breaks during the print. Be carefull to not damage the square base as it is needed to keep the key from turning in the keyboard housing.
* Test: The key base shall fit in the upper row of the keyboard.

3. Print "Button V3.3mf"
These are the key base for the middle row of the keyboard. There are 8  pieces and you will need them all. There are also 4 key-caps and you need to print some more as you need a total of 26. Be carefull to not damage the square base as it is needed to keep the key from turning in the keyboard housing.
* Test: The key base shall fit in the middle row of the keyboard.

4. Print "Button V2.3mf"
These are the key base for the lower row of the keyboard. There are 4  pieces and you will need 9 of them. To get them, print this file 3 times (then you have some spare). There are also 8 key-caps and if you print this file 3 times you have enough key-caps (see "Button V3.3mf") for the whole keyboard. Be carefull to not damage the square base as it is needed to keep the key from turning in the keyboard housing.
* Test: The key base shall fit in the lower row of the keyboard.

**********  Change filament to Silk Silver ***********
5. Print "Tastenkappe V1_20x.3mf"
This file  will produce 20 Key Cap Cover. Print the file twice so you have some spare if they get broken or lost. You will need 26 at least.
Pay attention to not install the Key Cap Cover upside down. They should not need glue.

----------------------------------------------------
Print Steckerbrett cover
Printer Prusa MK4, Filament PLA Black
----------------------------------------------------

1. Print "EIN-AUS_Schalter.3mf"
This is the switch-on/switch-off extention. The original one is to short when the steckerbrett cover is in place.

2. Print "Blende_Rechts.3mf"
This is the right side cover of the steckerbrett. Must be glued to the steckerbrett cover.

3. Print "Blende_Links.3mf"
This is the left side cover of the steckerbrett. Must be glued to the steckerbrett cover.

4. Print "Steckerbrett V2 Abschlusskante.3mf"
This is to cover the gap between the keyboard and the steckerbrett cover. Must be glued to the steckerbrett cover.

5. Print "Steckerbrett Magnethalter.3mf"
These two block must be fitted during the print with a neodyn magnet 20x5x2mm nad the they must be glued to the inside of the steckerbrett cover at a suitable place. The "oposite" magnte 20x5x2mm must be glued to the steckerbrett PCB.

6. Print "Steckerbrett V3.3mf"
There is a filament change programmed just before the last layer is to be printed. The new color is for the Enigma logo and the letter on the steckerbrett. (I recommand Bronze as color).
